**OXFORD ENGINEERING ESTONIA**

**C.N.C. TURNING**

**DAEWOO PUMA 400MB LARGE TURNING CENTRE Full C Axis Live Tooling**

X = 560∅

Z = 1100mm & 2028 Bore 114 mm.   
All axes simultaneously controlled

**MAZAK QUICK TURN CNC Turning Centre**

Capacity 675mm Maximum Turning Dia. 538 mm between centres.  
350mm Maximum Dia over carriage.

**HITACHI SEIKI HI-TURNER CNC Lathe (x2)**

Capacity 8” Chucking x 52mm bore. Maximum turning diameter 350mm  
Hydrafeed short bar loader

**C.N.C. MILLING**

**HAAS VF4 VERTICAL MACHINING CENTRE with high speed spindle**

X = 1016

Y = 508 mm

Fully integrated fourth axis control,   
Haas control system 20 tool capacity automatic   
changer

**BRIDGEPORT EZ-Trak - Mill**

X=762mm

Y=305mm

Z=220mm

**HAAS VF3 VERTICAL MACHINING CENTRE (x2)**

with fully integrated fourth axis control  
X = 1016

Y = 508 mm  
20 tool capacity automatic changer

**ROKU ROKU VERTICAL MACHINING CENTRE**

X = 765mm

Y = 410mm

Z = 510mm  
Fanuc 6M control system, 24 tool carousel

**HAAS VF0 VERTICAL MACHINING CENTER**

X = 510mm  
Y = 400mm   
Z = 400mm

20 tools, 10000 RPM

**Miyano TSV35 VERTICAL MACHINING CENTER**

X = 500mm   
Y = 380mm   
Z = 250mm

12 tools, 6000RPM

**CONVENTIONAL/SEMI AUTOMATIC TURNING**

**Colchester centre lathe 10" chuck**

**OTHER FACILITIES**

**Industrial Marking Machine PROPEN P5000PN**

**INSPECTION**

**ABERLINK CMM AXIOM TOO 640mmx600mmx500mm**